002 Saniplus

The original macerator for a full bathroom

* ***For full bathroom applications***
* ***↑ 15 Ft ↑ and/or ← 150 Ft →***

For more information:

<https://www.saniflo.com/us/installing-a-toilet/73-saniplus.html>

005 Toilet Tank White

SANIFLO's two-piece toilet systems for use with **Saniaccess 2, Saniaccess 3, Saniplus and Sanibest Pro**

* ***EPA WaterSense listed***
* ***Elongated bowl is ADA compliant***
* ***Includes soft-close toilet seat***

For more information:

<https://www.saniflo.com/us/accessories/227-round-and-elongated-rear-discharge-toilets.html>

008 Sanivite

Drain pump for kitchen installation or for any gray water application

* ***For commercial or residential applications***
* ***↑ 16 Ft ↑ and/or ← 150 Ft →***
* ***Perfect quiet solution***
* ***Capability to handle hot water and grease buildup***

Top of Form

﻿For more information:

<https://www.saniflo.com/us/installing-an-additional-bathroom/96-sanivite.html>Bottom of Form

010 Sanishower

Residential drain pump for gray water applications

* ***For medium-duty applications***
* ***↑ 12 Ft ↑ and/or ← 100 Ft →***
* ***Small enough to fit underneath a shower base***

For more information:

<https://www.saniflo.com/us/installing-an-additional-bathroom/94-sanishower.html>

011 Sanipack

The perfect solution for a full bathroom with style.

* ***For full bathroom applications***
* ***↑ 15 Ft ↑ and/or ← 150 Ft →***
* ***Use any wall-hung toilet to complete your bathroom installation***

Top of Form

﻿ For more information:

<https://www.saniflo.com/us/installing-a-toilet/162-sanipack.html>

012 Sanistar

A self-contained macerating wall-hung toilet

* ***For half-bathroom applications***
* ***↑ 9 Ft ↑ and/or ← 100 Ft →***
* ***Toilet with built-in macerating system***
* ***Water saving dual-flush system***

***For more information:***

<https://www.saniflo.com/us/installing-a-toilet/78-sanistar.html>

Bottom of Form

013 Sanibest Pro

The Sanibest Pro is the best solution to install a full bathroom in demanding situations.

* ***For full bathroom applications***
* ***↑ 25 Ft ↑ and/or ← 150 Ft →***
* ***Grinder system designed to handle sanitary products***
* ***Easy access service panel***

For more information:

<https://www.saniflo.com/us/installing-a-toilet/69-sanibest-pro.html>

014 Sanigrind Pro

The Sanigrind Pro is the best solution to install a full bathroom in demanding situations using any conventional toilet.

* ***For full bathroom applications***
* ***↑ 25 Ft ↑ and/or ← 150 Ft →***
* ***Grinder system designed to handle sanitary products***
* ***Easy access service panel***

Top of Form

﻿For more information:

<https://www.saniflo.com/us/installing-a-toilet/224-sanigrind-pro.html>

018 Sanicom 1

Heavy-duty drain pump for applications requiring gray water removal

* ***For commercial applications***
* ***↑ 25 Ft ↑ and/or ← 250 Ft →***
* ***Can handle multiple fixtures simultaneously***
* ***Capable of handling up to 194°F***

For more information:

<https://www.saniflo.com/us/installing-a-kitchen-or-laundry-room/102-sanicom-1.html>

020 Sanicompact Comfort

SANICOMPACT COMFORT is a wall-hung toilet with a built-in macerator. With its modern design and economical flush system, it will fit into any bathroom.

* ***For half-bathroom applications***
* ***↑ 9 Ft ↑ and/or ← 120 Ft →***
* ***Toilet with built-in macerating system***
* ***Water saving dual-flush system***

021 Saniswift

An easy solution for a remote laundry room installation or for any gray water application

* ***Residential drain pump***
* ***↑ 14 Ft ↑ and/or ← 140 Ft →***
* ***Compact design***
* ***Powerful and economical***

For more information:

<https://www.saniflo.com/us/installing-a-kitchen-or-laundry-room/225-saniswift.html>

023 Sanicompact

A self-contained macerating toilet for small spaces.

* ***For half-bathroom applications***
* ***↑ 9 Ft ↑ and/or ← 120 Ft →***
* ***Toilet with built-in macerating system***
* ***Water saving dual-flush system***

For more information:

<https://www.saniflo.com/us/home/74-sanicompact.html>

029 Sanicubic 2 240v

A pre-assembled duplex grinder system capable of discharging wastewater from multiple fixtures

* ***↑ 36 Ft ↑ and/or ← 328 Ft  →***
* ***Two powerful 1 HP motors***
* ***Grinder system designed to handle sanitary products***
* ***Rated IP68 with external control and alarm***
* ***Easy-access service panels***
* ***Capable of handling up to 90 GPM***

For more information:

<https://www.saniflo.com/us/installing-a-lifting-station/106-sanicubic-2-classic.html>

030 Extension Pipe

**Ideal Use:** Behind wall installation of Saniflo Pumps

040 Sanicondens

The easy solution to pump condensate away from condensing boilers and air conditioners

* ***Suitable for a condensing boiler, HVAC systems, air conditioners***
* ***↑ 15 Ft ↑ and/or ← 150 Ft →***

For more information:

<https://www.saniflo.com/us/installing-a-boiler-or-air-conditioner/85-sanicondens.html>

041 Sanicondens Best

2-in-1 condensate pump which neutralizes and pumps away condensate

* ***Built-in neutralizer to raise pH levels for harsh HVAC applications***
* ***↑ 15 Ft ↑ and/or ← 150 Ft →***
* ***Equipped with all necessary hardware for easy installation***

For more information:

<https://www.saniflo.com/us/installing-a-boiler-or-air-conditioner/82-sanicondens-best.html>

042 Sanicondens Best Neutralizer

Neutralizing granules To be used with SaniCondens best system Model # 042 Works with model #041 Neutralizer raises pH levels for harsh HVAC applications Used to refill SaniFlo model #041.

043 Sanineutral

A system that neutralizes acidic condensate from condensing boilers, HVAC systems, water heater systems, etc.

For more information:

<https://www.saniflo.com/us/installing-a-boiler-or-air-conditioner/86-sanineutral.html>

044 Sanicondens Best Flat

2-in-1 low profile condensate pump which neutralizes and pumps away condensate.

* ***Built-in neutralizer to raise pH levels for harsh HVAC applications***
* ***↑ 15 Ft ↑ and/or ← 150 Ft →***
* ***500,000 BTU per hour***
* ***Equipped with all necessary hardware for easy installation***

049 Sanicubic 1 VX 240v

A pre-assembled simplex lift station with Vortex impeller, capable of discharging wastewater from multiple fixtures.

* ***↑ 36 Ft (2'') or 20 Ft (4'') ↑***
* ***Powerful 1.5 HP motor***
* ***Vortex system designed to handle sanitary products and large diameter solids***
* ***Rated IP68 with external control and alarm***
* ***Easy-access service panels***

For more information:

<https://www.saniflo.com/us/installing-a-lifting-station/230-sanicubic-1-vx.html>

050 Sanialarm

Our macerators and gray water pumps are designed for various types of applications. Therefore, they are exposed to different situations such as power failures, occasional abuse, or build-ups of limescale deposits in older units (if not regularly descaled) which can cause a surcharge of water in the unit.

* ***Alerts of high water levels inside the pump***
* ***Helps prevent inappropriate use***
* ***Encourages prompt intervention***

For more information:

<https://www.saniflo.com/us/accessories/211-sanialarm.html>

052 Descaler

Regular descaling with specially formulated SANIFLO descaler will prolong the unit's life and maintain optimum performance.  It is specifically created for use with Saniflo products and laboratory formulated with phosphoric acid.  Regular usage prolongs unit life, maintains efficiency and it is harmless to septic tank operation.

Top of Form

﻿For more Information:

<https://www.saniflo.com/us/accessories/210-descaler.html>

081 Saniaccess 2

The Saniaccess 2 is ideal to create an additional half-bathroom anywhere.

* ***For half-bathroom applications***
* ***↑ 15 Ft ↑ and/or ← 150 Ft →***
* ***Quietest pump on the market***
* ***Easy dual-access service panels***

For more information:

<https://www.saniflo.com/us/installing-a-toilet/67-saniaccess-2.html>

082 Saniaccess 3

The most advanced macerator in the world with dual accessibility

* ***For full bathroom applications***
* ***↑ 15 Ft ↑ and/or ← 150 Ft →***
* ***Easy dual-access service panels***

For more Information:

<https://www.saniflo.com/us/installing-a-toilet/68-saniaccess-3.html>

Bottom of Form

083 Toilet Bowl Round White

SANIFLO's two-piece toilet systems for use with **Saniaccess 2, Saniaccess 3, Saniplus and Sanibest Pro**

* ***EPA WaterSense listed***
* ***Elongated bowl is ADA compliant***
* ***Includes soft-close toilet seat***

For more information:

<https://www.saniflo.com/us/accessories/227-round-and-elongated-rear-discharge-toilets.html>

087 Toilet Bowl Enlongated White

SANIFLO's two-piece toilet systems for use with **Saniaccess 2, Saniaccess 3, Saniplus and Sanibest Pro**

* ***EPA WaterSense listed***
* ***Elongated bowl is ADA compliant***
* ***Includes soft-close toilet seat***

For more information:

<https://www.saniflo.com/us/accessories/227-round-and-elongated-rear-discharge-toilets.html>

089 Sanicubic 1 120v

069 Sanicubic 1 240v

A pre-assembled simplex grinder system capable of discharging wastewater from multiple fixtures

* ***↑ 36 Ft ↑ and/or ← 328 Ft →***
* ***Powerful 1 HP motor***
* ***Grinder system designed to handle sanitary products***
* ***Rated IP68 with external control and alarm***
* ***Easy-access service panels***
* ***Also available in 240V (Part# 069)***

For more information:

<https://www.saniflo.com/us/installing-a-lifting-station/105-sanicubic-1.html>

099 Sanicubic 2 VX 240v

A pre-assembled duplex Vortex lift station capable of discharging wastewater from multiple fixtures

* ***↑ 36 Ft (2'') or 20 Ft (4'') ↑***
* ***Two powerful 1.5 HP motors***
* ***Vortex system designed to handle sanitary products and large diameter solids***
* ***Rated IP68 with external control and alarm***
* ***Easy-access service panels***

Top of Form

Bottom of FormFor more information:

<https://www.saniflo.com/us/installing-a-lifting-station/230-sanicubic-1-vx.html>

Bottom of Form